****

CERTIFICATE OF ANALYSIS

PRODUCT DESCRIPTION: Buffered Phosphate Dilution Water Item No.: 3024-25

VOLUME 5 gallon LOT No. 171602 EXP. DATE 09/2017

|  |  |  |  |
| --- | --- | --- | --- |
| TEST | RESULTS | SPECIFICATION | METHOD |
| pH | 7.2 | 7.2 ± 0.2 | WS cSOP 8.0 |
| TOXICITY \* | Count at 0 minutes: 36Count at 45 minutes: 35 | < 20 % decrease | WS cSOP 24.3 |
| FILL VOLUME | CONFORMS | LABEL | WS SOP CP3024-25.2.2 |
| COLOR | CONFORMS | CLEAR, COLORLESS,NO FOREIGN MATTER | VISUAL |
| PACKAGEINTEGRITYJERRYCAN | CONFORMS | NO LOOSE CAPSNO LEAKAGE | VISUAL |
| PACKAGE MARKINGS | CONFORMS | CONFORMSTO WS STD | WS SOP CP3024-25.4.0 |
| WATERQUALITY | CONFORMS | MICROBIO-LOGICALLY SUITABLE | *SMEWW*TABLE 9020:II |

Reference: *Standard Methods for the Examination of Dairy Products,* 17th edition, 2004, 4.020 – 4.042; *Standard Methods for the Examination of Water and Wastewater*, 20th edition

 \*TEST PERFORMED AT COMMERCIAL LAB: New Jersey Laboratories

**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Made By:

Weber Scientific

2732 Kuser Road

Hamilton, NJ 08691

(609)-584-7677

 Fred Weber

President

 Date *October 19, 2016*